**KARACHI SHIPYARD & ENGINEERING WORKS LIMITED**

Ref: SB/SC/INSU-CLAD/SB-287/2025 Dated: 03-02-2025

**INVITATION OF PROPOSALS & QUOTATION**

1. Proposals and sealed quotations are invited from well reputed Sub-Contractors / Firms who have the experience of Marine Insulation and Cladding Work onboard ship. Details are as under:

|  |  |  |
| --- | --- | --- |
| **SB MBU-1** | **DESCRIPTION** | **SPECIFICATION** |
| KS&EW Order No.  SB-287 | Insulation and Cladding work on Exhaust Pipes of ME(s), DG(s) & Gas Turbines of vessel under construction. | As per details given in tender documents available in the office of Development & Sub-Contract, Works Office Building, Ship Planning Hall (SB Division) |

2. Sub-Contractor shall use efficient tools / devices / equipment during Insulation and Cladding Installation / alignment processes for ensuring Quality and Product.

3. Required Tender Document may be obtained from office of Development & Sub-Contract (Ground Floor, Ship Planning Hall, Works Office Building), Telephone: 99214045-64 Extension No**.464** on any working day (Monday to Friday) between 0900 to 1600 hours, before bidding, on payment of tender fee of Rs.2000/- (Non-Refundable). Tender document can be obtained from 12-02-2025. The bidders must submit their offer before 1100 Hours on 05-03-2025 in single package envelope containing / comprising two separate sealed envelopes:

1. One envelope shall contain **“TECHNICAL PROPOSAL”** with Pre-Qualification form for Sub-Contractor with signature and office stamp of Sub-Contractor.
2. Second envelope contains **“COMMERCIAL / FINANCIAL PROPOSAL”.**

4. Accordingly Technical Proposal will be opened on the same date (i.e. 05-03-2025) at 1130 hours in the office of Development & Sub-Contract in presence of bidders who wish to be present. The commercial / financial proposal will be opened in presence of only technically qualified bidders on the date intimated by KS&EW later on.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

MAHBOOB HUSSAIN KHAN

DGM (Deck & Hold)

